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Eyewash Station Inspection Form
	Station ID/Location: ______________________________

	To pass inspection, the eyewash station must meet the following criteria:
Water is flowing steadily to allow rinsing of the facial area.
Water must be clean after running for least a full minute to determine the condition of the source.
Access to the eyewash station is unobstructed.
Eyewash station has been wiped down.
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