[image: ]

Ladder Inspection Checklist

	Inspector Name: 
	Date:

	Ladder ID:
	Company Name:

	Type: ☐ Step ☐ Portable ☐ Extension ☐ Other
	Material: ☐ Wood ☐ Metal ☐ Portable ☐ Plastic ☐ Other




Answer the following questions, marking any non-applicable ones as “yes.” If you answer any questions with “no,” do not use the ladder. Make sure to tag it out or fix the issue before putting it back into service.
General
	Ladder sits evenly on the ground without any wobble.
	☐ Yes   ☐ No

	All screws are firmly secured.
	☐ Yes   ☐ No

	Ladder is clean and free of slippery or sticky substances.
	☐ Yes   ☐ No

	End caps are present, whole, and free of cracks or tears.
	☐ Yes   ☐ No 

	There are no sharp areas on the ladder.
	☐ Yes   ☐ No 

	All rungs and steps are tightly fixed and free of cracks.
	☐ Yes   ☐ No 

	Non-slip materials on rungs, rails, and steps are in good shape.
	☐ Yes   ☐ No 

	All rungs are free of rust and residue.
	☐ Yes   ☐ No 

	There is no missing hardware (screws, hinges, bolts, etc.).
	☐ Yes   ☐ No 

	Spreaders are in place, functional, and free of defects.
	☐ Yes   ☐ No 

	Ladder has a warning label that operators can both see and read.
	☐ Yes   ☐ No 


Portable/Foldable/Extendable
	Hinges close all the way with a reasonable amount of force.
	☐ Yes   ☐ No

	Lock system engages correctly and fastens securely.
	☐ Yes   ☐ No

	Platform is in working order and all surrounding guards/rails are secure.
	☐ Yes   ☐ No

	Pulley system works properly and doesn’t have any frayed ropes.
	☐ Yes   ☐ No 

	The ladder has visible instructions for proper use.
	☐ Yes   ☐ No 

	Ladder has a functional guide system for safe extension.
	☐ Yes   ☐ No 



Notes:
2
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