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HVAC Inspection Checklist

	AREA OF CONCERN
	CONDITION
	NOTES

	Evaporator coils
	☐ Good ☐ Fair ☐ Poor
	 

	Condenser coils
	☐ Good ☐ Fair ☐ Poor
	

	Compressor contactor
	☐ Good ☐ Fair ☐ Poor
	

	Start capacitor
	☐ Good ☐ Fair ☐ Poor
	

	Pressure switch
	☐ Good ☐ Fair ☐ Poor
	

	Gauges
	☐ Good ☐ Fair ☐ Poor
	

	System lubrication
	☐ Good ☐ Fair ☐ Poor
	

	Thermostat
	☐ Good ☐ Fair ☐ Poor
	

	Air filters
	☐ Good ☐ Fair ☐ Poor
	

	Electrical connections
	☐ Good ☐ Fair ☐ Poor
	

	Blower motor amp draw
	☐ Good ☐ Fair ☐ Poor
	

	Blower belts
	☐ Good ☐ Fair ☐ Poor
	

	Condenser motor amp draw
	☐ Good ☐ Fair ☐ Poor
	

	Refrigerant levels
	☐ Good ☐ Fair ☐ Poor
	

	Crankcase heater
	☐ Good ☐ Fair ☐ Poor
	

	Compressors
	☐ Good ☐ Fair ☐ Poor
	

	Condensation drain and pan
	☐ Good ☐ Fair ☐ Poor
	

	Defrost controls
	☐ Good ☐ Fair ☐ Poor
	

	Coil temperature
	☐ Good ☐ Fair ☐ Poor
	

	Reversing valves
	☐ Good ☐ Fair ☐ Poor
	

	Heat sequencer
	☒ Good ☐ Fair ☐ Poor
	

	Bearings
	☐ Good ☐ Fair ☐ Poor
	

	Heat anticipator
	☐ Good ☐ Fair ☐ Poor
	

	Electrical wiring
	☐ Good ☐ Fair ☐ Poor
	

	Temperature rise
	☐ Good ☐ Fair ☐ Poor
	

	Supply temperature
	☐ Good ☐ Fair ☐ Poor
	

	Ductwork
	☐ Good ☐ Fair ☐ Poor
	

	Flue system
	☐ Good ☐ Fair ☐ Poor
	

	Pilot/ignition system
	☐ Good ☐ Fair ☐ Poor
	

	Burners
	☐ Good ☐ Fair ☐ Poor
	

	Blower motor
	☐ Good ☐ Fair ☐ Poor
	

	Manifold pressure
	☐ Good ☐ Fair ☐ Poor
	

	Fan controls
	☐ Good ☐ Fair ☐ Poor
	



Notes on the overall condition of the HVAC system:
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